

1. **Host software：**

The mainframe is connected to the computer through a data cable.

1、Double-click to open the software




2、Drop down to select the corresponding port



3、Software interface

After entering the interface, press the “Read” key to read the original data.



Area A**：**

* Startup Text: Enter the content to change the display name of the host secondary menu.
* Language：The language of the host can be set, and Chinese / English is supported.
* ID：The host ID, can be changed to support the value 1000-2000 (the last digit must be 0).


Note: after changing the ID, it must be re-paired with the extension before you can continue to use it later.

Area B**：**The host displays the function menu settings, and if you check it, the host will display the following menu accordingly.

* ：STUDYCAPCODE
* ：SET FLASH LED ENABLE/SET FLASH LED DISABLE
* ：SET BEEP ENABLE/SET BEEP DISABLE
* ：SET VIBRATE ENABLE/SET VIBRATE DISABLE
* ： SET REMIND VOICE ENABLE/ SET REMIND VOICE DISABLE
* ：SET ALERT LENGTH： 1-30 secs.
* ：SET RESET BY CHARGER/ SET RESET NO CHARGER  The menu is not displayed, but the default information is sent with the "0" key when the text is sent.
* ：SET LOGO(Refers to the contents displayed when the menu is turned on.)
* ：SET FLASH RESET BY CHARGER DISABLE/ SET FLASH RESET BY CHARGER ENABLE
* ：SET OUT OF RANGE DISABLE
* ：SET OUT OF RANGE TIME(2-9): value: 2-9 （Minute），"OUT" will be displayed when the time is exceeded.
* : SET OUT OF RANGE ALERT INTERVAL TIME(1-9): value 1-9（Minute）
* : SET CHECK RSSI ENABLE/ SET CHECK RSSI DISABLE
* ：SET ZOOM 1/SET ZOOM 2/SET ZOOM 3(Set font size)
* : Set up the group call function

Area C**：**Custom numeric button (0MI9) send content by default (up to 32 characters in Chinese / 64 characters in English).


1. **Extension software**
2. Double-click to open the software



2. Select the port and enter the user name + password


The port is selected as: COM Port (Auto).

User name, password: admin




3. Enter the meal license number to be called.

The address code is the number to be called, and the number of the meal plate with 4 digits in 1966, for example, meal plate No. 1, is: 1960001.



4. Enter the content and send

Enter what you need to send at 1 (up to 32 characters in Chinese / 64 characters in English) and then press icon 2 to send



Contact Email: [support@retekess.com](mailto:support@retekess.com)

Website: [www.retekess.com](http://www.retekess.com)